* There may be no more than 55 gallons of hazardous waste (or 1 liter of acutely toxic waste) at this SAA at any one time.
	+ If there is, the Lab Manager/PI must contact Research Compliance at (575-517-0646 or hazmat@nmt.edu) who must relocate the waste to the Central Accumulation Area (CAA) within exactly three days.
* All waste must be labeled upon generation.
	+ Use Hazardous Waste Labels provided by Research Compliance. Make sure to add chemical names (NOT FORMULAS) and concentrations.
	+ Add initial date of waste generation under “Satellite Accumulation Area Start Date”.
	+ DO NOT add a date to the “Central Accumulation Area Start Date”. Research Compliance will fill this out when the waste is transported to the CAA.
* Store incompatible wastes separately.
* Keep lids securely on containers when not actively adding waste.